**Postponement Procedure**

Description of Flag:

AP Answering Pennant

Red and White Vertical Stripes

POSTPONEMENT SHALL BEMADE PRIOR TO THE START

CONDITIONS:

1. Lack of wind.

2. Inability to notify VTS.

3. Significant error in timing sequence.

SEQUENCE:

1. Postponement Flag Up with TWO GUNS OR SOUND SIGNALS.
2. When it is decided to resume the sequence, Postponement Flag Down with ONE GUN OR SOUND SIGNAL.
3. Wait ONE MINUTE.
4. Resume the Starting Sequence.

COMMENTS:

This signal ONLY affects those classes which HAVE NOT started.

"AP" over "H" means 'All races not started are postponed. Further signals ashore.’

"AP" over "A" means 'All races not started are postponedto a later day.'